|  |
| --- |
| Truck Carrying Capacities for Mulch |
| ½ Ton Short Bed Pickup  | 2 Cubic yards |
| ½ or ¾ Ton Long Bed Pickup | 2.5 Cubic yards |
| Ranger Type Pickup | 1.5 Cubic yards |

Visit Landscapecalculator.com

for easy auto calculation!

Note: There are 27 cubic feet in one cubic yard!

|  |
| --- |
| Material Coverage in Cubic Yards |
| **ft2 To Cover** | **1” Deep** | **2” Deep** | **3” Deep** | **4” Deep** | **5” Deep** | **6” Deep** |
| **50** | .15 | .3 | .46 | .62 | .78 | .93 |
| **100** | .3 | .62 | .93 | 1.24 | 1.54 | 1.85 |
| **200** | .61 | 1.23 | 1.85 | 2.47 | 3.09 | 3.7 |
| **250** | .77 | 1.54 | 2.3 | 3.09 | 3.86 | 4.63 |
| **300** | .92 | 1.85 | 2.78 | 3.7 | 4.63 | 5.6 |
| **400** | 1.2 | 2.5 | 3.7 | 4.94 | 6.2 | 7.41 |
| **500** | 1.5 | 3 | 4.63 | 6.2 | 7.72 | 9.23 |
| **1000** | 3.1 | 6.2 | 9.26 | 12.35 | 15.43 | 18.52 |

|  |
| --- |
| Bag Coverage |
| **Bag Size** | **Depth** | **Coverage Per Bag (ft2)** | **# of Bags Required to Cover** |
| **8’ x 8’** **64 ft2** | **25’ x 4’** **100 ft2** | **12’ x 12’****144 ft2** |
| **1 Cubic Ft** | 2” | 6 | 11 | 17 | 24 |
| 3” | 4 | 16 | 25 | 36 |
| 4” | 2 | 22 | 33 | 48 |
| **2 Cubic Ft** | 2” | 12 | 6 | 9 | 12 |
| 3” | 8 | 8 | 13 | 18 |
| 4” | 6 | 11 | 17 | 24 |
| **3 Cubic Ft** | 2” | 18 | 4 | 6 | 8 |
| 3” | 12 | 6 | 9 | 12 |
| 4” | 9 | 8 | 12 | 16 |